ADD_RAM_OUTPUT_REGISTER=OFF
INTENDED_DEVICE_FAMILY="Cyclone V"
LPM_NUMWORDS=256
LPM_SHOWAHEAD=OFF
LPM_TYPE=scfifo
LPM_WIDTH=8
LPM_WIDTHU=8
OVERFLOW_CHECKING=ON
UNDERFLOW_CHECKING=ON
USE_EAB=ON
DEVICE_FAMILY="Cyclone V"
clock
data
rdreq
wrreq
empty
full
q
usedw
